<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="28.626" y2="0" width="0" layer="20"/>
<wire x1="28.626" y1="0" x2="28.626" y2="49.52" width="0" layer="20"/>
<wire x1="28.626" y1="49.52" x2="0" y2="49.52" width="0" layer="20"/>
<wire x1="0" y1="49.52" x2="0" y2="0" width="0" layer="20"/>
<hole x="2.54" y="46.736" drill="3.2"/>
<hole x="26.0858" y="46.736" drill="3.2"/>
<hole x="26.0858" y="2.54" drill="3.2"/>
<hole x="2.54" y="2.54" drill="3.2"/>
<text>GND</text>
<text>2</text>
<text>1</text>
<text>OUT</text>
<text>IN</text>
<text>1</text>
<text>2</text>
<text>GND</text>
<text>5V</text>
<text>GND</text>
<text>5V</text>
<text>5V</text>
<text>GND</text>
<text>5V</text>
<text>comma pedal</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_NO_SILK_YES_STOP">
</package>
</packages>
</library>
<library name="comma.ai">
<packages>
<package name="LQFP64">
<description>Based on STM PCB landpattern recomendation</description>
</package>
<package name="HVSON8">
</package>
<package name="XTAL-3.2X2.5">
</package>
<package name="0402-R">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0603-C">
</package>
<package name="USB-A-S">
<description>&lt;b&gt;USB Series A Surface Mounted&lt;/b&gt;</description>
</package>
<package name="RA-RJ45">
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="oldlib">
<description>MobileEye connector</description>
<packages>
<package name="LOGO">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="comma.ai" package="0603-C" value="2.2uF">
<attribute name="NAME"/>
</element>
<element name="C10" library="comma.ai" package="0603-C" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C11" library="comma.ai" package="0603-C" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C12" library="comma.ai" package="0603-C" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="C13" library="comma.ai" package="0603-C" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C15" library="comma.ai" package="0603-C" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C16" library="comma.ai" package="0603-C" value="2.2uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="comma.ai" package="0603-C" value="2.2uF">
<attribute name="NAME"/>
</element>
<element name="C26" library="comma.ai" package="0603-C" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C3" library="comma.ai" package="0603-C" value="12pF">
<attribute name="NAME"/>
</element>
<element name="C4" library="comma.ai" package="0603-C" value="12pF">
<attribute name="NAME"/>
</element>
<element name="C8" library="comma.ai" package="0603-C" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C9" library="comma.ai" package="0603-C" value="100nF">
<attribute name="NAME"/>
</element>
<element name="LED1" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J15" library="comma.ai" package="RA-RJ45" value="RJ45 to OBDII">
<attribute name="NAME"/>
</element>
<element name="R1" library="comma.ai" package="0402-R" value="10k">
<attribute name="NAME"/>
</element>
<element name="R13" library="comma.ai" package="0402-R" value="220">
<attribute name="NAME"/>
</element>
<element name="R16" library="comma.ai" package="0402-R" value="22">
<attribute name="NAME"/>
</element>
<element name="R17" library="comma.ai" package="0402-R" value="22">
<attribute name="NAME"/>
</element>
<element name="R2" library="comma.ai" package="0402-R" value="10k">
<attribute name="NAME"/>
</element>
<element name="R23" library="comma.ai" package="0402-R" value="1k">
<attribute name="NAME"/>
</element>
<element name="R24" library="comma.ai" package="0402-R" value="1k">
<attribute name="NAME"/>
</element>
<element name="R25" library="comma.ai" package="0402-R" value="1k">
<attribute name="NAME"/>
</element>
<element name="R26" library="comma.ai" package="0402-R" value="1k">
<attribute name="NAME"/>
</element>
<element name="R3" library="comma.ai" package="0402-R" value="10k">
<attribute name="NAME"/>
</element>
<element name="R4" library="comma.ai" package="0402-R" value="10k">
<attribute name="NAME"/>
</element>
<element name="U1" library="comma.ai" package="LQFP64" value="STM32-M-64-LQFP"/>
<element name="U2" library="SparkFun-PowerIC" package="SOT23-5" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="VREG-00822"/>
<attribute name="VALUE"/>
</element>
<element name="U6" library="comma.ai" package="SO08" value="MCP6002">
<attribute name="NAME"/>
</element>
<element name="Y1" library="comma.ai" package="XTAL-3.2X2.5" value="16MHz">
<attribute name="NAME"/>
</element>
<element name="R7" library="comma.ai" package="0402-R" value="10k">
<attribute name="NAME"/>
</element>
<element name="R8" library="comma.ai" package="0402-R" value="10k">
<attribute name="NAME"/>
</element>
<element name="U3" library="comma.ai" package="HVSON8" value="TJA1042HVSON">
<attribute name="NAME"/>
</element>
<element name="C5" library="comma.ai" package="0603-C" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C6" library="comma.ai" package="0603-C" value="100nF">
<attribute name="NAME"/>
</element>
<element name="R5" library="comma.ai" package="0402-R" value="10k">
<attribute name="NAME"/>
</element>
<element name="R6" library="comma.ai" package="0402-R" value="10k">
<attribute name="NAME"/>
</element>
<element name="J3" library="comma.ai" package="USB-A-S" value="USB-ASMD-F">
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X06_NO_SILK_YES_STOP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X06_NO_SILK_YES_STOP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="oldlib" package="LOGO" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="63"/>
<contactref element="U1" pad="28"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U1" pad="12"/>
<contactref element="C13" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="U6" pad="4"/>
<contactref element="C26" pad="2"/>
<contactref element="R26" pad="2"/>
<contactref element="R25" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="U3" pad="2"/>
<contactref element="U3" pad="PAD"/>
<contactref element="J15" pad="1"/>
<contactref element="J15" pad="5"/>
<contactref element="Y1" pad="4"/>
<contactref element="Y1" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="J3" pad="GND"/>
<contactref element="J1" pad="5"/>
<contactref element="J1" pad="2"/>
<contactref element="J2" pad="5"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="VCAP2">
<contactref element="U1" pad="47"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="VCAP1">
<contactref element="U1" pad="31"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="3V3">
<contactref element="U1" pad="13"/>
<contactref element="C13" pad="1"/>
<contactref element="U1" pad="64"/>
<contactref element="U1" pad="19"/>
<contactref element="U1" pad="48"/>
<contactref element="U1" pad="32"/>
<contactref element="C8" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="U2" pad="5"/>
<contactref element="C16" pad="1"/>
<contactref element="LED1" pad="A"/>
<contactref element="U3" pad="5"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="C3" pad="1"/>
<contactref element="Y1" pad="1"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="Y1" pad="3"/>
<contactref element="C4" pad="1"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="5V">
<contactref element="U6" pad="8"/>
<contactref element="C26" pad="1"/>
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="U3" pad="3"/>
<contactref element="C5" pad="1"/>
<contactref element="J3" pad="VBUS"/>
<contactref element="J1" pad="4"/>
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="4"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="CAN1_RX">
<contactref element="U1" pad="61"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="CAN1_TX">
<contactref element="U1" pad="62"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="CAN1_EN">
<contactref element="U1" pad="55"/>
<contactref element="U3" pad="8"/>
</signal>
<signal name="BOOT0">
<contactref element="U1" pad="60"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="U1" pad="20"/>
<contactref element="U6" pad="3"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="U6" pad="5"/>
<contactref element="U1" pad="21"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="DAC1">
<contactref element="U6" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="DAC2">
<contactref element="U6" pad="7"/>
<contactref element="R2" pad="2"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$21">
<contactref element="U6" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="R2" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="U6" pad="6"/>
</signal>
<signal name="N$41">
<contactref element="R23" pad="1"/>
<contactref element="R26" pad="1"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="N$42">
<contactref element="R24" pad="1"/>
<contactref element="U1" pad="9"/>
<contactref element="R25" pad="1"/>
</signal>
<signal name="ACCEL1">
<contactref element="R23" pad="2"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="ACCEL2">
<contactref element="R24" pad="2"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$26">
<contactref element="LED1" pad="C"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="C15" pad="1"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="45"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R16" pad="1"/>
<contactref element="U1" pad="44"/>
</signal>
<signal name="N$5">
<contactref element="R16" pad="2"/>
<contactref element="J3" pad="D-"/>
</signal>
<signal name="N$6">
<contactref element="R17" pad="2"/>
<contactref element="J3" pad="D+"/>
</signal>
<signal name="LEDG">
<contactref element="U1" pad="30"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="CAN1_L">
<contactref element="U3" pad="6"/>
<contactref element="J15" pad="3"/>
</signal>
<signal name="CAN1_H">
<contactref element="U3" pad="7"/>
<contactref element="J15" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="R5" pad="2"/>
<contactref element="J3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
