(kicad_pcb (version 20171130) (host pcbnew 5.0.2+dfsg1-1~bpo9+1)
  (general
    (thickness 1.6)
    (drawings 38)
    (tracks 1244)
    (zones 0)
    (modules 82)
    (nets 92)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 150 100)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/home/jhaupt/Projects/Cellphone/Electrical/Fab/"))
  )
  (net 0 "")
  (net 1 /RESET)
  (net 2 GND)
  (net 3 /AREF)
  (net 4 +5V)
  (net 5 "Net-(C7-Pad1)")
  (net 6 "Net-(C8-Pad1)")
  (net 7 "Net-(C9-Pad1)")
  (net 8 "Net-(C10-Pad2)")
  (net 9 "Net-(C11-Pad1)")
  (net 10 +BATT)
  (net 11 "Net-(D1-Pad2)")
  (net 12 "Net-(D2-Pad2)")
  (net 13 "Net-(D3-Pad1)")
  (net 14 "Net-(D4-Pad2)")
  (net 15 "Net-(D4-Pad1)")
  (net 16 "Net-(D5-Pad1)")
  (net 17 "Net-(D5-Pad2)")
  (net 18 "Net-(D6-Pad2)")
  (net 19 "Net-(D7-Pad2)")
  (net 20 "Net-(D8-Pad2)")
  (net 21 "Net-(D9-Pad2)")
  (net 22 "Net-(D10-Pad2)")
  (net 23 "Net-(D11-Pad2)")
  (net 24 "Net-(D12-Pad2)")
  (net 25 "Net-(D13-Pad2)")
  (net 26 "Net-(D14-Pad2)")
  (net 27 "Net-(D15-Pad2)")
  (net 28 /MISO)
  (net 29 /MOSI)
  (net 30 /SCK)
  (net 31 "/USB PORT AND BRIDGE/ATMEGA-TX_TO_FTDI-RX")
  (net 32 "/USB PORT AND BRIDGE/ATMEGA-RX_TO_FTDI-TX")
  (net 33 "Net-(J1-Pad13)")
  (net 34 "Net-(J1-Pad14)")
  (net 35 "Net-(J2-Pad1)")
  (net 36 "Net-(Q2-Pad1)")
  (net 37 "Net-(R2-Pad1)")
  (net 38 "Net-(R6-Pad1)")
  (net 39 "Net-(R7-Pad1)")
  (net 40 "Net-(R8-Pad1)")
  (net 41 "Net-(R9-Pad2)")
  (net 42 "Net-(U1-Pad10)")
  (net 43 "/Vibration Motor Circuit/VIB_PWM")
  (net 44 /+631)
  (net 45 /NoPrepend)
  (net 46 /AltKey)
  (net 47 "Net-(J1-Pad11)")
  (net 48 "Net-(J1-Pad12)")
  (net 49 "Net-(J1-Pad15)")
  (net 50 "Net-(J1-Pad16)")
  (net 51 "Net-(J1-Pad17)")
  (net 52 "Net-(J1-Pad18)")
  (net 53 "Net-(J1-Pad6)")
  (net 54 "Net-(J1-Pad7)")
  (net 55 "Net-(J1-Pad9)")
  (net 56 "Net-(R2-Pad2)")
  (net 57 "Net-(R3-Pad2)")
  (net 58 "Net-(R4-Pad2)")
  (net 59 "Net-(R5-Pad2)")
  (net 60 "Net-(R12-Pad1)")
  (net 61 "Net-(R13-Pad2)")
  (net 62 "Net-(R14-Pad2)")
  (net 63 "Net-(R15-Pad2)")
  (net 64 "Net-(R16-Pad2)")
  (net 65 "Net-(R17-Pad2)")
  (net 66 "Net-(R18-Pad2)")
  (net 67 "Net-(R19-Pad2)")
  (net 68 "Net-(R20-Pad2)")
  (net 69 "Net-(R21-Pad2)")
  (net 70 "Net-(R22-Pad2)")
  (net 71 "Net-(R23-Pad2)")
  (net 72 "Net-(R24-Pad2)")
  (net 73 "Net-(R25-Pad2)")
  (net 74 "Net-(SW3-Pad1)")
  (net 75 "Net-(SW4-Pad1)")
  (net 76 "Net-(SW5-Pad1)")
  (net 77 "Net-(SW6-Pad1)")
  (net 78 "Net-(SW7-Pad1)")
  (net 79 "Net-(SW8-Pad1)")
  (net 80 "Net-(U2-Pad2)")
  (net 81 "Net-(U3-Pad12)")
  (net 82 "Net-(U3-Pad11)")
  (net 83 "Net-(U3-Pad10)")
  (net 84 "Net-(U3-Pad9)")
  (net 85 "Net-(U3-Pad8)")
  (net 86 "Net-(U3-Pad7)")
  (net 87 "Net-(J3-Pad1)")
  (net 88 "Net-(J3-Pad2)")
  (net 89 "Net-(J3-Pad3)")
  (net 90 "Net-(J3-Pad4)")
  (net 91 "Net-(J3-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net +BATT)
    (add_net /+631)
    (add_net /AREF)
    (add_net /AltKey)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /NoPrepend)
    (add_net /RESET)
    (add_net /SCK)
    (add_net "/USB PORT AND BRIDGE/ATMEGA-RX_TO_FTDI-TX")
    (add_net "/USB PORT AND BRIDGE/ATMEGA-TX_TO_FTDI-RX")
    (add_net "/Vibration Motor Circuit/VIB_PWM")
    (add_net GND)
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad2)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D14-Pad2)")
    (add_net "Net-(D15-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R18-Pad2)")
    (add_net "Net-(R19-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R20-Pad2)")
    (add_net "Net-(R21-Pad2)")
    (add_net "Net-(R22-Pad2)")
    (add_net "Net-(R23-Pad2)")
    (add_net "Net-(R24-Pad2)")
    (add_net "Net-(R25-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(SW3-Pad1)")
    (add_net "Net-(SW4-Pad1)")
    (add_net "Net-(SW5-Pad1)")
    (add_net "Net-(SW6-Pad1)")
    (add_net "Net-(SW7-Pad1)")
    (add_net "Net-(SW8-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U3-Pad10)")
    (add_net "Net-(U3-Pad11)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U3-Pad8)")
    (add_net "Net-(U3-Pad9)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.9)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J2-Pad1)")
  )
  (module MyFootprints:Adafruit_eInkFriendBreakout (layer F.Cu) (tedit 5E10F223)
    (at 141.75 75.5)
    (fp_text reference U3 (at 17.75 -19) (layer F.SilkS))
    (fp_text value eInkBreakoutFriendHeader (at 0.5 -6) (layer F.Fab))
    (fp_text user ENA (at -13.97 -2.032 90) (layer F.SilkS))
    (fp_text user BUSY (at -11.43 -2.54 90) (layer F.SilkS))
    (fp_text user RST (at -8.89 -2.032 90) (layer F.SilkS))
    (fp_text user SRCS (at -6.35 -2.54 90) (layer F.SilkS))
    (fp_text user D/C (at -3.81 -2.54 90) (layer F.SilkS))
    (fp_text user ECS (at -1.27 -2.032 90) (layer F.SilkS))
    (fp_text user MOSI (at 1.27 -2.54 90) (layer F.SilkS))
    (fp_text user MISO (at 3.81 -2.54 90) (layer F.SilkS))
    (fp_text user SCK (at 6.35 -2.032 90) (layer F.SilkS))
    (fp_text user GND (at 8.89 -2.032 90) (layer F.SilkS))
    (fp_text user 3V3 (at 11.43 -2.032 90) (layer F.SilkS))
    (fp_text user Vin (at 13.97 -2.032 90) (layer F.SilkS))
    (pad 12 thru_hole circle (at -13.97 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 81 "Net-(U3-Pad12)"))
    (pad 11 thru_hole circle (at -11.43 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 82 "Net-(U3-Pad11)"))
    (pad 10 thru_hole circle (at -8.89 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 83 "Net-(U3-Pad10)"))
    (pad 9 thru_hole circle (at -6.35 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 84 "Net-(U3-Pad9)"))
    (pad 8 thru_hole circle (at -3.81 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 85 "Net-(U3-Pad8)"))
    (pad 7 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 86 "Net-(U3-Pad7)"))
    (pad 6 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 /MOSI))
    (pad 5 thru_hole circle (at 3.81 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 /MISO))
    (pad 4 thru_hole circle (at 6.35 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 /SCK))
    (pad 3 thru_hole circle (at 8.89 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 11.43 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 13.97 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 +BATT))
  )
  (module MyFootprints:FONA_3G (layer F.Cu) (tedit 5E10AEC2)
    (at 138.25 129.75 270)
    (fp_text reference J1 (at -24 19.75 270) (layer F.SilkS))
    (fp_text value FONA3G_Daughterboard (at 0 19.05 270) (layer F.Fab))
    (fp_text user -SPKR (at -21.59 19.685) (layer F.SilkS))
    (fp_text user +SPKR (at -19.05 19.685) (layer F.SilkS))
    (fp_text user -MIC (at -16.51 20.32) (layer F.SilkS))
    (fp_text user NS (at -11.43 20.955) (layer F.SilkS))
    (fp_text user +MIC (at -13.97 20.32) (layer F.SilkS))
    (fp_text user RI (at -6.35 20.955) (layer F.SilkS))
    (fp_text user PS (at -8.89 20.955) (layer F.SilkS))
    (fp_text user KEY (at -3.81 20.955) (layer F.SilkS))
    (fp_text user CTS (at -1.27 20.955) (layer F.SilkS))
    (fp_text user DTR (at 1.27 20.955) (layer F.SilkS))
    (fp_text user RTS (at 3.81 20.955) (layer F.SilkS))
    (fp_text user Tx (at 6.35 20.955) (layer F.SilkS))
    (fp_text user Rx (at 8.89 20.955) (layer F.SilkS))
    (fp_text user Rst (at 11.43 20.955) (layer F.SilkS))
    (fp_text user Vio (at 13.97 20.955) (layer F.SilkS))
    (fp_text user GND (at 16.51 20.955) (layer F.SilkS))
    (fp_text user BATT (at 19.05 20.32) (layer F.SilkS))
    (fp_text user 5V (at 21.59 20.955) (layer F.SilkS))
    (pad 1 thru_hole circle (at 21.59 22.987 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 2 thru_hole circle (at 19.05 22.987 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 +BATT))
    (pad 3 thru_hole circle (at 16.51 22.987 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 13.97 22.987 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 +BATT))
    (pad 5 thru_hole circle (at 11.43 22.987 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 8.89 22.987 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 53 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at 6.35 22.987 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 54 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at 3.81 22.987 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 1.27 22.987 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 55 "Net-(J1-Pad9)"))
    (pad 10 thru_hole circle (at -1.27 22.987 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at -3.81 22.987 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 47 "Net-(J1-Pad11)"))
    (pad 12 thru_hole circle (at -6.35 22.987 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 48 "Net-(J1-Pad12)"))
    (pad 13 thru_hole circle (at -8.89 22.987 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 "Net-(J1-Pad13)"))
    (pad 14 thru_hole circle (at -11.43 22.987 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad14)"))
    (pad 15 thru_hole circle (at -13.97 22.987 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 49 "Net-(J1-Pad15)"))
    (pad 16 thru_hole circle (at -16.51 22.987 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 50 "Net-(J1-Pad16)"))
    (pad 17 thru_hole circle (at -19.05 22.987 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 51 "Net-(J1-Pad17)"))
    (pad 18 thru_hole circle (at -21.59 22.987 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 52 "Net-(J1-Pad18)"))
  )
  (module MyFootprints:TQFP-100_14x14mm_P0.5mm (layer F.Cu) (tedit 5E1144E9)
    (at 130.5 138 90)
    (descr "TQFP, 100 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_qfp_generator.py")
    (tags "TQFP QFP")
    (attr smd)
    (fp_text reference U4 (at 0 -9.35 90) (layer F.SilkS))
    (fp_text value ATmega2560V-8AU (at 0 9.35 90) (layer F.Fab))
    (fp_text user %R (at 0 0.5 90) (layer F.Fab))
    (pad 100 smd rect (at -6 -7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 10 +BATT))
    (pad 99 smd rect (at -5.5 -7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 98 smd rect (at -5 -7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 /AREF))
    (pad 97 smd rect (at -4.5 -7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(R24-Pad2)"))
    (pad 96 smd rect (at -4 -7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(J1-Pad9)"))
    (pad 95 smd rect (at -3.5 -7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(R13-Pad2)"))
    (pad 94 smd rect (at -3 -7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(R25-Pad2)"))
    (pad 93 smd rect (at -2.5 -7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 92 smd rect (at -2 -7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 91 smd rect (at -1.5 -7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 90 smd rect (at -1 -7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 89 smd rect (at -0.5 -7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 88 smd rect (at 0 -7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 87 smd rect (at 0.5 -7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 86 smd rect (at 1 -7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(J3-Pad5)"))
    (pad 85 smd rect (at 1.5 -7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(J3-Pad4)"))
    (pad 84 smd rect (at 2 -7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(J3-Pad3)"))
    (pad 83 smd rect (at 2.5 -7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(J3-Pad2)"))
    (pad 82 smd rect (at 3 -7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(J3-Pad1)"))
    (pad 81 smd rect (at 3.5 -7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 80 smd rect (at 4 -7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 10 +BATT))
    (pad 79 smd rect (at 4.5 -7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 78 smd rect (at 5 -7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 77 smd rect (at 5.5 -7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 76 smd rect (at 6 -7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(R12-Pad1)"))
    (pad 75 smd rect (at 7.65 -6 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(U3-Pad7)"))
    (pad 74 smd rect (at 7.65 -5.5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(U3-Pad8)"))
    (pad 73 smd rect (at 7.65 -5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(U3-Pad9)"))
    (pad 72 smd rect (at 7.65 -4.5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(U3-Pad10)"))
    (pad 71 smd rect (at 7.65 -4 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(U3-Pad11)"))
    (pad 70 smd rect (at 7.65 -3.5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U2-Pad2)"))
    (pad 69 smd rect (at 7.65 -3 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 68 smd rect (at 7.65 -2.5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 67 smd rect (at 7.65 -2 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 66 smd rect (at 7.65 -1.5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 65 smd rect (at 7.65 -1 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 64 smd rect (at 7.65 -0.5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(R19-Pad2)"))
    (pad 63 smd rect (at 7.65 0 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R18-Pad2)"))
    (pad 62 smd rect (at 7.65 0.5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 61 smd rect (at 7.65 1 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 +BATT))
    (pad 60 smd rect (at 7.65 1.5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 59 smd rect (at 7.65 2 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(U3-Pad12)"))
    (pad 58 smd rect (at 7.65 2.5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(SW8-Pad1)"))
    (pad 57 smd rect (at 7.65 3 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(SW7-Pad1)"))
    (pad 56 smd rect (at 7.65 3.5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(SW6-Pad1)"))
    (pad 55 smd rect (at 7.65 4 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(SW5-Pad1)"))
    (pad 54 smd rect (at 7.65 4.5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(SW4-Pad1)"))
    (pad 53 smd rect (at 7.65 5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(SW3-Pad1)"))
    (pad 52 smd rect (at 7.65 5.5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 51 smd rect (at 7.65 6 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 50 smd rect (at 6 7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 49 smd rect (at 5.5 7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 48 smd rect (at 5 7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 47 smd rect (at 4.5 7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 46 smd rect (at 4 7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 46 /AltKey))
    (pad 45 smd rect (at 3.5 7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 45 /NoPrepend))
    (pad 44 smd rect (at 3 7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 44 /+631))
    (pad 43 smd rect (at 2.5 7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 2 7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(R17-Pad2)"))
    (pad 41 smd rect (at 1.5 7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(R16-Pad2)"))
    (pad 40 smd rect (at 1 7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 0.5 7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 38 smd rect (at 0 7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 37 smd rect (at -0.5 7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(R15-Pad2)"))
    (pad 36 smd rect (at -1 7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(R14-Pad2)"))
    (pad 35 smd rect (at -1.5 7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(R5-Pad2)"))
    (pad 34 smd rect (at -2 7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(R2-Pad2)"))
    (pad 33 smd rect (at -2.5 7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(R3-Pad2)"))
    (pad 32 smd rect (at -3 7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 31 smd rect (at -3.5 7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 10 +BATT))
    (pad 30 smd rect (at -4 7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /RESET))
    (pad 29 smd rect (at -4.5 7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd rect (at -5 7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at -5.5 7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd rect (at -6 7.65 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(R4-Pad2)"))
    (pad 25 smd rect (at -7.65 6 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at -7.65 5.5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at -7.65 5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at -7.65 4.5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 28 /MISO))
    (pad 21 smd rect (at -7.65 4 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MOSI))
    (pad 20 smd rect (at -7.65 3.5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 30 /SCK))
    (pad 19 smd rect (at -7.65 3 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(J1-Pad7)"))
    (pad 18 smd rect (at -7.65 2.5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(J1-Pad6)"))
    (pad 17 smd rect (at -7.65 2 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -7.65 1.5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(R23-Pad2)"))
    (pad 15 smd rect (at -7.65 1 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(R22-Pad2)"))
    (pad 14 smd rect (at -7.65 0.5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -7.65 0 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(R21-Pad2)"))
    (pad 12 smd rect (at -7.65 -0.5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(R20-Pad2)"))
    (pad 11 smd rect (at -7.65 -1 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at -7.65 -1.5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 +BATT))
    (pad 9 smd rect (at -7.65 -2 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -7.65 -2.5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -7.65 -3 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -7.65 -3.5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -7.65 -4 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 43 "/Vibration Motor Circuit/VIB_PWM"))
    (pad 4 smd rect (at -7.65 -4.5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -7.65 -5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 31 "/USB PORT AND BRIDGE/ATMEGA-TX_TO_FTDI-RX"))
    (pad 2 smd rect (at -7.65 -5.5 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 32 "/USB PORT AND BRIDGE/ATMEGA-RX_TO_FTDI-TX"))
    (pad 1 smd rect (at -7.65 -6 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/TQFP-100_14x14mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyFootprints:Trimline_RotaryDial_Terminals (layer F.Cu) (tedit 5E10CB55)
    (at 150 99.6)
    (fp_text reference U2 (at 6.15 21.3) (layer F.SilkS))
    (fp_text value Rotary_Dial (at 9.75 31.9) (layer F.Fab))
    (pad 1 thru_hole circle (at 9 26) (size 7 7) (drill 3.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 15.2 20.3) (size 7 7) (drill 3.5) (layers *.Cu *.Mask)
      (net 80 "Net-(U2-Pad2)"))
  )
  (module MyFootprints:Everlight-12-21SYGCS530-E2TR8 (layer B.Cu) (tedit 5E10A282)
    (at 126.75 146 62)
    (fp_text reference D1 (at 3.470418 0.136744 62) (layer B.SilkS))
    (fp_text value LED (at 0 -7.5 62) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0.25 62) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.499999 0.25 62) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(D1-Pad2)"))
  )
  (module MyFootprints:Everlight-12-21SYGCS530-E2TR8 (layer B.Cu) (tedit 5E10A282)
    (at 121 142.5 56)
    (fp_text reference D2 (at 3.470576 0.674612 56) (layer B.SilkS))
    (fp_text value LED (at 0 -7.5 56) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0.25 56) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0.25 56) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(D2-Pad2)"))
  )
  (module MyFootprints:Everlight-12-21SYGCS530-E2TR8 (layer B.Cu) (tedit 5E10A282)
    (at 179.681836 125.832682 90)
    (fp_text reference D6 (at -3.417318 0.568164 90) (layer B.SilkS))
    (fp_text value LED (at 0 -7.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0.25 90) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0.25 90) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(D6-Pad2)"))
  )
  (module MyFootprints:Everlight-12-21SYGCS530-E2TR8 (layer B.Cu) (tedit 5E10A282)
    (at 179.681836 120.082682 90)
    (fp_text reference D7 (at 0.5 -1.5 90) (layer B.SilkS))
    (fp_text value LED (at 0 -7.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0.25 90) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0.25 90) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(D7-Pad2)"))
  )
  (module MyFootprints:Everlight-12-21SYGCS530-E2TR8 (layer B.Cu) (tedit 5E10A282)
    (at 179.681836 114.332682 90)
    (fp_text reference D8 (at 1.832682 -1.681836 90) (layer B.SilkS))
    (fp_text value LED (at 0 -7.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0.25 90) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0.25 90) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(D8-Pad2)"))
  )
  (module MyFootprints:Everlight-12-21SYGCS530-E2TR8 (layer B.Cu) (tedit 5E10A282)
    (at 179.681836 108.582682 90)
    (fp_text reference D9 (at 0.082682 -1.5 90) (layer B.SilkS))
    (fp_text value LED (at 0 -7.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0.25 90) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0.25 90) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(D9-Pad2)"))
  )
  (module MyFootprints:Everlight-12-21SYGCS530-E2TR8 (layer B.Cu) (tedit 5E10A282)
    (at 179.681836 102.832682 90)
    (fp_text reference D10 (at -0.667318 -2.181836 180) (layer B.SilkS))
    (fp_text value LED (at 0 -7.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0.25 90) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0.25 90) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(D10-Pad2)"))
  )
  (module MyFootprints:Everlight-12-21SYGCS530-E2TR8 (layer B.Cu) (tedit 5E10A282)
    (at 179.681836 97.082682 90)
    (fp_text reference D11 (at -0.917318 -2.181836 180) (layer B.SilkS))
    (fp_text value LED (at 0 -7.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0.25 90) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0.25 90) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(D11-Pad2)"))
  )
  (module MyFootprints:Everlight-12-21SYGCS530-E2TR8 (layer B.Cu) (tedit 5E10A282)
    (at 179.681836 91.332682 90)
    (fp_text reference D12 (at -1.667318 -2.181836 180) (layer B.SilkS))
    (fp_text value LED (at 0 -7.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0.25 90) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0.25 90) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(D12-Pad2)"))
  )
  (module MyFootprints:Everlight-12-21SYGCS530-E2TR8 (layer B.Cu) (tedit 5E10A282)
    (at 179.681836 85.582682 90)
    (fp_text reference D13 (at -1.417318 -2.181836 180) (layer B.SilkS))
    (fp_text value LED (at 0 -7.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0.25 90) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0.25 90) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(D13-Pad2)"))
  )
  (module MyFootprints:Everlight-12-21SYGCS530-E2TR8 (layer B.Cu) (tedit 5E10A282)
    (at 179.681836 79.832682 90)
    (fp_text reference D14 (at -1.167318 -2.181836 180) (layer B.SilkS))
    (fp_text value LED (at 0 -7.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0.25 90) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0.25 90) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(D14-Pad2)"))
  )
  (module MyFootprints:Everlight-12-21SYGCS530-E2TR8 (layer B.Cu) (tedit 5E10A282)
    (at 179.681836 74.082682 90)
    (fp_text reference D15 (at 0.5 -1.5 90) (layer B.SilkS))
    (fp_text value LED (at 0 -7.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0.25 90) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0.25 90) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(D15-Pad2)"))
  )
  (module MyFootprints:ICSP_Header (layer F.Cu) (tedit 5BD65D9F)
    (at 171 136.75 315)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -3.889087 -6.363961 45) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0 -3.1 315) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 -2.5 315) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 /MISO))
    (pad 2 thru_hole oval (at 2.54 -2.5 315) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 +BATT))
    (pad 3 thru_hole oval (at 0 0.04 315) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 /SCK))
    (pad 4 thru_hole oval (at 2.54 0.04 315) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 /MOSI))
    (pad 5 thru_hole oval (at 0 2.579999 315) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /RESET))
    (pad 6 thru_hole oval (at 2.54 2.58 315) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (offset (xyz 1.269999980926514 -2.539999961853027 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5E120D6E)
    (at 120.5 120.25 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R25 (at 0 -1.25 270) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(R25-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(J1-Pad14)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 143 136)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /RESET))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 121.25 148.375 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 -1.43 270) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /AREF))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 172.75 126.25 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0 -1.43 270) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 +BATT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 164.875 58.25)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 0.25 -1.5) (layer B.SilkS))
    (fp_text value .1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 +BATT))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 134 118 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 0.25 -1.5 90) (layer B.SilkS))
    (fp_text value .1uF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 +BATT))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 124.75 96.5 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at 0 -1.43 180) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.874999 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.874999 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 +BATT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 145.5 145 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at 0 1.43 180) (layer B.SilkS))
    (fp_text value 10nF (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 152.5 139.5 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C8 (at 1.5 1.5 90) (layer B.SilkS))
    (fp_text value 47pF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C8-Pad1)"))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 150.5 139.5 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C9 (at 0 1.43 270) (layer B.SilkS))
    (fp_text value 47pF (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 145.5 144)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C10 (at 0 -1.43) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /RESET))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C10-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 152 67)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C11 (at 0 1.43) (layer B.SilkS))
    (fp_text value .1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 161 143)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D3 (at 0.25 2) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Castellated (layer F.Cu) (tedit 5B301BBE)
    (at 160.8125 137.5)
    (descr "LED SMD 0603 (1608 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED castellated")
    (attr smd)
    (fp_text reference D4 (at 0 -1.38) (layer F.SilkS))
    (fp_text value LED (at 0 1.38) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.8125 0) (size 1.225 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(D4-Pad2)"))
    (pad 1 smd roundrect (at -0.8125 0) (size 1.225 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric_Castellated.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Castellated (layer F.Cu) (tedit 5B301BBE)
    (at 165 133.25)
    (descr "LED SMD 0603 (1608 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED castellated")
    (attr smd)
    (fp_text reference D5 (at 2.5 0) (layer F.SilkS))
    (fp_text value LED (at 0 1.38) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.8125 0) (size 1.225 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(D5-Pad1)"))
    (pad 2 smd roundrect (at 0.8125 0) (size 1.225 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric_Castellated.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer B.Cu) (tedit 58645DC7)
    (at 163.5 66 180)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D16 (at 1 2 180) (layer B.SilkS))
    (fp_text value D_Schottky (at 0 -2.1 180) (layer B.Fab))
    (fp_text user %R (at 0 2 180) (layer B.Fab))
    (pad 2 smd rect (at 1.65 0 180) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.65 0 180) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyFootprints:JST-PH_RA (layer F.Cu) (tedit 5CE74552)
    (at 176.5 82 180)
    (fp_text reference J2 (at 0 -3 180) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0.5 -3 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 3.5) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 3.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -3.4 5.6 180) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 3.4 5.6 180) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 156 143.5 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference L1 (at 2.25 -0.25) (layer F.SilkS))
    (fp_text value Ferrite_Bead (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 13 "Net-(D3-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyFootprints:SMT_VibrationMotor (layer B.Cu) (tedit 5CE8B0F4)
    (at 140 69)
    (fp_text reference M1 (at -1 3.5) (layer B.SilkS))
    (fp_text value Motor_DC (at 0.25 -4.5) (layer B.Fab))
    (pad 1 smd rect (at -3.75 2) (size 3 2) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at -3.75 -2) (size 3 2) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 148.75 132.5 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference MK1 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value "Elecret Microphone" (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 -180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(J1-Pad16)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(J1-Pad15)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyFootprints:AMPHENOL_MicroUSB_10118194-0001LF (layer B.Cu) (tedit 5BBF63FB)
    (at 148 151.5 180)
    (attr smd)
    (fp_text reference P2 (at -5 2.5 90) (layer B.SilkS))
    (fp_text value USB_MICRO-B (at 5.27468 3.28101 90) (layer B.SilkS) hide)
    (fp_text user PCB~Edge (at 4.258539 -1.503017 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.3 2.675) (size 0.45 1.35) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at -0.65 2.675) (size 0.45 1.35) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C8-Pad1)"))
    (pad 3 smd rect (at 0 2.675) (size 0.45 1.35) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C9-Pad1)"))
    (pad 4 smd rect (at 0.65 2.675) (size 0.45 1.35) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 1.3 2.675) (size 0.45 1.35) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at -2.5 2.7 180) (size 1.408 1.408) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 2.5 2.7 180) (size 1.408 1.408) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at -3.5 0 180) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 3.5 0 180) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -1 0 180) (size 1.5 1.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 1 0 180) (size 1.5 1.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -3.05 0 180) (size 1.5 1.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 3.05 0 180) (size 1.5 1.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module MyFootprints:SuperSOT-3 (layer B.Cu) (tedit 5C7C8702)
    (at 136.5 60.5)
    (descr "3-pin SuperSOT package https://www.fairchildsemi.com/package-drawings/MA/MA03B.pdf")
    (tags "SuperSOT-3 SSOT-3")
    (attr smd)
    (fp_text reference Q2 (at 1 -3) (layer B.SilkS))
    (fp_text value FDN340P (at 0.1 -2.9 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 -1.1 270) (size 1.4 1) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at 0.95 -1.1 270) (size 1.4 1) (layers B.Cu B.Paste B.Mask)
      (net 10 +BATT))
    (pad 3 smd rect (at 0 1.1 270) (size 1.4 1) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SuperSOT-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 143.125 139 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.43 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /RESET))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 +BATT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 127.75 138.125 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at -1.375 -1.25 90) (layer B.SilkS))
    (fp_text value 1M (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(R2-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 130.5 138.125 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0.75 1.43 90) (layer B.SilkS))
    (fp_text value 27R (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(R2-Pad1)"))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 133 145.75)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at -2.5 0.25) (layer B.SilkS))
    (fp_text value 2k (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(D1-Pad2)"))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 134 144)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0.125 -1.25) (layer B.SilkS))
    (fp_text value 2k (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(D2-Pad2)"))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 150.5 144 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 1.43 270) (layer B.SilkS))
    (fp_text value 27R (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C9-Pad1)"))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(R6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 152.5 144 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 1.5 -1.5 270) (layer B.SilkS))
    (fp_text value 27R (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C8-Pad1)"))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(R7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 125.5 149.25 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(R8-Pad1)"))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "/USB PORT AND BRIDGE/ATMEGA-RX_TO_FTDI-TX"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 135 149.75)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(R9-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "/USB PORT AND BRIDGE/ATMEGA-TX_TO_FTDI-RX"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 160.5 134)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 33k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0.433848) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 164.875 131)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 2k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(D5-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 120.5 130.125 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(J1-Pad12)"))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(R12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 118.25 121.875 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R13 (at 1.625 -1.25 270) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(J1-Pad13)"))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(R13-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 175.75 122.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R14 (at -0.25 1.25 180) (layer B.SilkS))
    (fp_text value 2k (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(D6-Pad2)"))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(R14-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 170.75 126 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R15 (at 1 1.43 180) (layer B.SilkS))
    (fp_text value 2k (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(R15-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(D7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 177 110.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R16 (at 1 1.5 180) (layer B.SilkS))
    (fp_text value 2k (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(R16-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(D8-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 176.875 106.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R17 (at 0 1.43 180) (layer B.SilkS))
    (fp_text value 2k (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(R17-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(D9-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 177 101.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R18 (at 1 1.43 180) (layer B.SilkS))
    (fp_text value 2k (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(D10-Pad2)"))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(R18-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 177 96 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R19 (at 1 1.43 180) (layer B.SilkS))
    (fp_text value 2k (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(D11-Pad2)"))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 67 "Net-(R19-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 177 90 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R20 (at 0.5 1.43 180) (layer B.SilkS))
    (fp_text value 2k (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(R20-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(D12-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 177 84.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R21 (at 1 1.43 180) (layer B.SilkS))
    (fp_text value 2k (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(R21-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(D13-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 177 78.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R22 (at 0 1.43 180) (layer B.SilkS))
    (fp_text value 2k (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(D14-Pad2)"))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(R22-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 176.625 71.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R23 (at 0 1.43 180) (layer B.SilkS))
    (fp_text value 2k (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(D15-Pad2)"))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(R23-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 124 81.625001 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R26 (at 0 -1.43 270) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.874999 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "/Vibration Motor Circuit/VIB_PWM"))
    (pad 1 smd roundrect (at -0.874999 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyFootprints:SP3T_OS103011MS8QP1 (layer B.Cu) (tedit 5CE8A6B5)
    (at 120 74 270)
    (fp_text reference SW1 (at 3.75 -5.5 270) (layer B.SilkS))
    (fp_text value SP3T (at 0.3 4.1 270) (layer B.Fab))
    (pad 1 thru_hole circle (at -4 -3.5 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 46 /AltKey))
    (pad 2 thru_hole circle (at 0 -3.5 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 2 -3.5 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 45 /NoPrepend))
    (pad 4 thru_hole circle (at 4 -3.5 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 44 /+631))
  )
  (module MyFootprints:SPDT (layer B.Cu) (tedit 5CE8A8EA)
    (at 121 91 270)
    (fp_text reference SW2 (at 1 -6.4 270) (layer B.SilkS))
    (fp_text value SW_SPDT (at 1 6.5 270) (layer B.Fab))
    (pad 1 thru_hole circle (at -2.5 -4.5 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 +BATT))
    (pad 2 thru_hole circle (at 0 -4.5 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad1)"))
    (pad 3 thru_hole circle (at 2.5 -4.5 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask))
  )
  (module MyFootprints:SSOP-16 (layer F.Cu) (tedit 5C7C7BEC)
    (at 150 138)
    (descr "SSOP 20 pins")
    (tags "CMS SSOP SMD")
    (attr smd)
    (fp_text reference U1 (at 4.25 -1.5) (layer F.SilkS))
    (fp_text value FT230XS (at -0.862 -0.008 270) (layer F.Fab))
    (pad 1 smd rect (at -2.767 -2.421 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at -2.767 -1.786 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C10-Pad2)"))
    (pad 3 smd rect (at -2.767 -1.1256 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U1-Pad10)"))
    (pad 4 smd rect (at -2.767 -0.4652 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R9-Pad2)"))
    (pad 5 smd rect (at -2.767 0.1698 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -2.767 0.8302 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -2.767 1.4906 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D5-Pad1)"))
    (pad 8 smd rect (at -2.767 2.1256 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R6-Pad1)"))
    (pad 9 smd rect (at 2.567 2.1256 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R7-Pad1)"))
    (pad 10 smd rect (at 2.567 1.4906 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U1-Pad10)"))
    (pad 11 smd rect (at 2.567 0.8302 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U1-Pad10)"))
    (pad 12 smd rect (at 2.567 0.1698 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 10 +BATT))
    (pad 13 smd rect (at 2.567 -0.4652 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at 2.567 -1.1256 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D4-Pad1)"))
    (pad 15 smd rect (at 2.567 -1.786 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 2.567 -2.421 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (model SMD_Packages.3dshapes/SSOP-20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.255 0.33 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyFootprints:AWSCR-16.00CV-T (layer B.Cu) (tedit 5BD5C24D)
    (at 122 148.75 180)
    (fp_text reference Y1 (at -3 -1 90) (layer B.SilkS))
    (fp_text value 8MHz (at 0.5 0.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 0.7 5) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(R2-Pad2)"))
    (pad 2 smd rect (at 0 0 180) (size 1 5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.5 0 180) (size 0.7 5) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(R2-Pad1)"))
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CEABC9D)
    (at 118.75 142.75)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R24 (at 1.5 1.25) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(J1-Pad11)"))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(R24-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_B3S-1000 (layer B.Cu) (tedit 5CF98A31)
    (at 160.5 137.5)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW3 (at 0 4.5) (layer B.SilkS))
    (fp_text value "Tactile Switch" (at 0 -4.5) (layer B.Fab))
    (fp_text user %R (at 0 4.5) (layer B.Fab))
    (pad 1 smd rect (at -3.975 2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 74 "Net-(SW3-Pad1)"))
    (pad 1 smd rect (at 3.975 2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 74 "Net-(SW3-Pad1)"))
    (pad 2 smd rect (at -3.975 -2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3.975 -2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_B3S-1000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_B3S-1000 (layer B.Cu) (tedit 5A02FC95)
    (at 172 62)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW4 (at 0 4.5) (layer B.SilkS))
    (fp_text value "Tactile Switch" (at 0 -4.5) (layer B.Fab))
    (fp_text user %R (at 0 4.5) (layer B.Fab))
    (pad 1 smd rect (at -3.975 2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 75 "Net-(SW4-Pad1)"))
    (pad 1 smd rect (at 3.975 2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 75 "Net-(SW4-Pad1)"))
    (pad 2 smd rect (at -3.975 -2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3.975 -2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_B3S-1000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_B3S-1000 (layer B.Cu) (tedit 5A02FC95)
    (at 139.5 137.5)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW5 (at 0 4.5) (layer B.SilkS))
    (fp_text value "Tactile Switch" (at 0 -4.5) (layer B.Fab))
    (fp_text user %R (at 0 4.5) (layer B.Fab))
    (pad 2 smd rect (at 3.975 -2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3.975 -2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 3.975 2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(SW5-Pad1)"))
    (pad 1 smd rect (at -3.975 2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(SW5-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_B3S-1000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_B3S-1000 (layer B.Cu) (tedit 5A02FC95)
    (at 173.75 131)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW6 (at 0 4.5) (layer B.SilkS))
    (fp_text value "Tactile Switch" (at 0 -4.5) (layer B.Fab))
    (fp_text user %R (at 0 4.5) (layer B.Fab))
    (pad 1 smd rect (at -3.975 2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 77 "Net-(SW6-Pad1)"))
    (pad 1 smd rect (at 3.975 2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 77 "Net-(SW6-Pad1)"))
    (pad 2 smd rect (at -3.975 -2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3.975 -2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_B3S-1000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_B3S-1000 (layer B.Cu) (tedit 5A02FC95)
    (at 128 62)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW7 (at 0 4.5) (layer B.SilkS))
    (fp_text value "Tactile Switch" (at 0 -4.5) (layer B.Fab))
    (fp_text user %R (at 0 4.5) (layer B.Fab))
    (pad 2 smd rect (at 3.975 -2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3.975 -2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 3.975 2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 78 "Net-(SW7-Pad1)"))
    (pad 1 smd rect (at -3.975 2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 78 "Net-(SW7-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_B3S-1000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_B3S-1000 (layer B.Cu) (tedit 5A02FC95)
    (at 126.25 131)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW8 (at 0 4.5) (layer B.SilkS))
    (fp_text value "Tactile Switch" (at 0 -4.5) (layer B.Fab))
    (fp_text user %R (at 0 4.5) (layer B.Fab))
    (pad 1 smd rect (at -3.975 2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 79 "Net-(SW8-Pad1)"))
    (pad 1 smd rect (at 3.975 2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 79 "Net-(SW8-Pad1)"))
    (pad 2 smd rect (at -3.975 -2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3.975 -2.25) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_B3S-1000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyFootprints:SP_DynamicSpeaker (layer B.Cu) (tedit 5E10A95E)
    (at 150 60.1 180)
    (fp_text reference LS1 (at -6 -6 180) (layer B.SilkS))
    (fp_text value Speaker (at 0.5 6 180) (layer B.Fab))
    (pad 1 smd rect (at -7.7 -3.9 180) (size 1.6 2.5) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(J1-Pad18)"))
    (pad 2 smd rect (at 7.7 -3.9 180) (size 1.6 2.5) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(J1-Pad17)"))
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 126 84.875 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R27 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(Q2-Pad1)"))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 +BATT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 5E114181)
    (at 121.5 62)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.25 -1.25) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 5E11417D)
    (at 165 62)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 5E114178)
    (at 115.75 104.25)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 5E114173)
    (at 176.5 125.5)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 5E11416D)
    (at 160.5 150.1)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 161.5 70 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J3 (at -0.5 12.5 90) (layer F.SilkS))
    (fp_text value Conn_01x05 (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 87 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "Net-(J3-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 "Net-(J3-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 "Net-(J3-Pad5)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 157.5 141) (end 157.5 153) (angle -45) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 169.5 129) (end 177.999999 137.499999) (angle -45) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 130 67) (end 130 55) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 169.5 67) (end 181.5 67) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_text "3.7v LiPoly" (at 176.5 66.75 270) (layer F.SilkS))
  (gr_text "FONA & eInk by Lady Ada" (at 120.25 85.5 270) (layer F.SilkS))
  (gr_text A11 (at 171.5 67 90) (layer F.SilkS))
  (gr_text A12 (at 169 67 90) (layer F.SilkS))
  (gr_text A13 (at 166.5 67 90) (layer F.SilkS))
  (gr_text A14 (at 164 67 90) (layer F.SilkS))
  (gr_text A15 (at 161.5 67 90) (layer F.SilkS))
  (gr_text GPIO (at 170 72.75) (layer F.SilkS))
  (gr_text "LIVE FREE OR DIE" (at 118 138 270) (layer B.SilkS))
  (gr_text Rx (at 160.5 139.5) (layer F.SilkS))
  (gr_line (start 113.5 102.25) (end 118 97.75) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166 149.5) (end 178 137.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 113.5 153) (end 157.5 153) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 113.5 102.25) (end 113.5 153) (layer Edge.Cuts) (width 0.15))
  (gr_text Tx (at 164.75 135.25) (layer F.SilkS))
  (gr_text "LIVE FREE OR DIE" (at 179.5 123 90) (layer F.SilkS))
  (gr_text "Cellphone by \nJustine Haupt" (at 177.5 99.5 90) (layer F.SilkS))
  (gr_line (start 136 107) (end 139 110) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.5 78) (end 129.5 78) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.5 77) (end 157.5 78) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.5 72.5) (end 158.5 77) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165.5 72.5) (end 158.5 72.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174 81) (end 165.5 72.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174 116) (end 174 81) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.5 116) (end 174 116) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.5 130) (end 160.5 116) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139 130) (end 146.5 130) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139 110) (end 139 130) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.5 107) (end 136 107) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 129.5 78) (end 129.5 107) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 181.5 67) (end 181.5 129) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130 55) (end 169.5 55) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118 67) (end 118 97.75) (layer Edge.Cuts) (width 0.2))
  (zone (net 10) (net_name +BATT) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.25 50) (xy 112.25 153.25) (xy 186 153.25) (xy 186 50)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.25 50) (xy 186 50) (xy 186 153.25) (xy 112.25 153.25)
      )
    )
  )
)
